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	SPECIFICATIONS 

  Working height (m)

  10.14

  Platform height (m)

  8.14

  Max. platform capacity (kg)

  450

  (A) Stowed Length (m)

  2.42

  (B) Overall width (m)

  1.20

  (C) Stowed height (guardrails) (m)

  2.26

  (D) Wheelbase (m)

  1.86

  (E) Ground clearance (cm)

  13

  (F) x (G) Max. platform size (m) (with extensions)

  3.22 x 1.20

  Weight (kg)

  2330

  Transport height (m)

  1.14

  Gradeability (%)

  23

  Power Source 

  240 AH Batteries

  Drive speed (high speed) (km/h)

  3

  Lift / lower speed (sec.)

  40 / 45

  Motricity

  4 x 2 x 2
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	SPECIFICATIONS 

  Working height (m)

  10

  Platform height (m)

  8

  Max. platform capacity (kg)

  230

  (A) Stowed Length (m)

  2.42

  (B) Overall width (m)

  0.81

  (C) Stowed height (guardrails) (m)

  2.25

  (D) Wheelbase (m)

  1.86

  (E) Ground clearance (cm)

  13

  (F) x (G) Max. platform size (m) (with extensions)

  3.22 x 0.80

  Weight (kg)

  2150

  Transport height (m)

  0.99

  Gradeability (%)

  25

  Power Source 

  209 AH Batteries

  Drive speed (high speed) (km/h)

  3

  Lift / lower speed (sec.)

  45 / 45

  Motricity

  4 x 2 x 2


	


	COMPACT 10 RTE - Sizes
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SPECIFICATIONS 

  Working height (m)

  10.2

  Platform height (m)

  8.2

  Max. platform capacity (kg)

  565

  (A) Stowed Length (m)

  2.65

  (B) Overall width (m)

  1.80

  (C) Stowed height (guardrails) (m)

  2.37

  (D) Wheelbase (m)

  1.87

  (E) Ground clearance (cm)

  25

  (F) x (G) Max. platform size (m) (with extensions)

  3.70 x 1.54

  Weight (kg)

  3380

  Transport height (m)

  1.3

  Gradeability (%)

  25

  Drive speed (high speed) (km/h)

  5.8

  Lift / lower speed (sec.)

  35 / 35

  Motricity

  4 x 2 x 2 




	COMPACT 12 - Sizes
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SPECIFICATIONS 

  Working height (m)

  12

  Platform height (m)

  10

  Max. platform capacity (kg)

  300

  (A) Stowed Length (m)

  2.42

  (B) Overall width (m)

  1.20

  (C) Stowed height (guardrails) (m)

  2.38

  (D) Wheelbase (m)

  1.86

  (E) Ground clearance (cm)

  13

  (F) x (G) Max. platform size (m) (with extensions)

  3.22 x 1.20

  Weight (kg)

  2630

  Transport height (m)

  1.26

  Gradeability (%)

  23

  Power Source 

  240 AH Batteries

  Drive speed (high speed) (km/h)

  3

  Lift / lower speed (sec.)

  45 / 50

  Motricity

  4 x 2 x 2
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	SPECIFICATIONS 

  Working height (m)

  12

  Platform height (m)

  10

  Max. platform capacity (kg)

  900

  (A) Stowed Length (m)

  4.12

  (B) Overall width (m)

  2.25

  (C) Stowed height (guardrails) (m)

  2.57

  (D) Wheelbase (m)

  2.75

  (E) Ground clearance (cm)

  35

  (F) x (G) Max. platform size (m) (with extensions)

  6 x 1.80

  Weight (kg)

  5350

  Transport height (m)

  1.71

  Gradeability (%)

  45

  Power Source 

  32 hp Diesel 

  Drive speed (high speed) (km/h)

  6

  Lift / lower speed (sec.)

  43 / 65

  Motricity

  4 x 4 x 2 
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SPECIFICATIONS 

  Working height (m)

  12.15

  Platform height (m)

  10.15

  Max. platform capacity (kg)

  450

  (A) Stowed Length (m)

  2.65

  (B) Overall width (m)

  1.80

  (C) Stowed height (guardrails) (m)

  2.54

  (D) Wheelbase (m)

  1.85

  (E) Ground clearance (cm)

  25

  (F) x (G) Max. platform size (m) (with extensions)

  3.70 x 1.54

  Weight (kg)

  3830

  Transport height (m)

  1.4

  Gradeability (%)

  40

  Power Source 

  24 hp Deutz diesel 

  Drive speed (high speed) (km/h)

  5.5

  Lift / lower speed (sec.)

  40 / 45

  Motricity

  4 x 4 x 2




