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YL9900MS Specifications 

1) Ion Source: ESI with APCI option (switchable with minimal effort)

2) API interface: orthogonal ion sampling from heated capillary – allows for small single turbo pump (Patents pending)

3) Flow rate range: 10 µL/min to 1mL/min (higher with simple split)

4) Polarity Switching: +ve and –ve ion in one single analysis
5) m/z Range: m/z 10 to m/z 1,200

6) Scan rate (Acquisition rate): 10,000 m/z units sec-1 (compatible with UHPLC)

7) Resolution: 0.5-0.7 m/z units (FWHM) at 1000 m/z units sec-1 over entire acquisition range

8) SIM sensitivity: 10 pg Reserpine (FIA – 5µL sample injection volume at 100 µL/min) 100:1 S/N (RMS) with SIM of m/z 609.28

9) Accuracy: ± 0.1 m/z units over entire acquisition range
10) Stability (m/x-units per 24hour period: 18 – 24oC): 0.1

11) Capillary Inlet: Exchange without breaking vaccum
[image: image1.jpg]